Standard Operating Procedure

Acrolein (2-Propenal)

**This is an SOP template and is not complete until: 1) lab specific information is entered into the box below 2) lab specific protocol/procedure is added to the protocol/procedure section and
3) SOP has been signed and dated by the PI and relevant lab personnel.**

Print a copy and insert into your *Lab-Specific Chemical Hygiene Plan*.

**Section 1 – Lab-Specific Information**

| **Building/Room(s) covered by this SOP:** | Click here to enter text. |
| --- | --- |
| **Department:** | Click here to enter a date. |
| **Principal Investigator Name:** | Click here to enter text. |
| **Principal Investigator Signature:** | Click here to enter text. |

**Section 2 – Hazards**

Acrolein is a highly flammable liquid, acutely toxic by oral ingestion, inhalation, and skin absorption. It is also corrosive, likely to be carcinogenic, and a reproductive toxin. Acrolein is fatal if swallowed or inhaled; and if in contact with skin or eyes, acrolein causes severe skin burns and eye damage. Symptoms of exposure are cough, shortness of breath, headache, and nausea.

**Exposure Limits:**

OSHA PEL (8 HR. TWA): 0.1 ppm



**Section 3 – Engineering Controls and Personal Protective Equipment (PPE)**

**Engineering Controls:** Acrolein must be used in a properly functioning chemical fume hood or glove box. The chemical fume hood must be approved and certified by REM and have a face velocity between 80 – 125 feet per minute.

**Hygiene Measures:** Avoid contact with skin, eyes, and clothing. Wash hands before breaks and immediately after handling the product.

**Hand Protection:** Chemical-resistant gloves must be worn, butyl-rubber gloves are recommended for handling acrolein. **NOTE:** Consult with your preferred glove manufacturer to ensure that the gloves you plan on using are compatible with the specific chemical being used.

**Eye Protection:** ANSI approved properly fitting safety glasses or chemical splash goggles are required.

**Skin and Body Protection:** Laboratory coats must be worn and be appropriately sized for the individual and buttoned to their full length. Flame resistant lab coats must be worn when handling volumes greater than 1 liter. Personnel must also wear full length pants, or equivalent, and close-toed shoes. Full length pants and close-toed shoes must be worn at all times by all individuals that are occupying the laboratory area. The area of skin between the shoe and ankle must not be exposed.

**Respiratory Protection:** If acrolein is being used outside of a chemical fume hood, respiratory protection is required. If the respirator is the sole means of protection, use a full-face supplied air respirator. If this activity is necessary, contact REM (49-46371) so a respiratory protection analysis can be performed.

**Section 4 – Special Handling and Storage Requirements**

* A designated storage area must be established for acrolein and the area should be posted with a “Caution, Carcinogen, Reproductive Toxins, or Extremely Toxic Chemicals” label provided by REM (as shown to the right).
* Do not over purchase; only purchase what can be safely stored in the laboratory.
* Avoid contact with skin, eyes, and inhalation.
* Keep away from sources of ignition.
* Keep containers tightly closed.
* Store in a cool, dry and well-ventilated area away from incompatible substances such as oxidizers.
* A suitable storage location is a flammable storage cabinet that does not contain incompatibles such as oxidizing agents, and strong acids or bases.

**Section 5 – Spill and Accident Procedures**

Immediately evacuate area and ensure others are aware of the spill. If there is an imminent threat of a fire, pull the nearest fire alarm station to evacuate the building and **dial 911**. If personnel have become exposed and need medical assistance, **dial 911**. If the spill is minor and does not pose a threat to personnel, contact REM at 49-40121 during normal business hours (Monday – Friday, 7 AM – 4 PM) for spill cleanup assistance (dial 911 if spill occurs after hours and assistance is needed).

**Section 6 – Waste Disposal Procedures**

All acrolein waste must be collected for proper waste disposal by REM (sink disposal is not permitted). Store hazardous waste in closed containers that are properly labeled, and in a designated area (flammable cabinet is recommended). Complete a Chemical Waste Pickup Request Form to arrange for disposal by REM; detailed instructions are provided at the following link: <http://www.purdue.edu/ehps/rem/hmm/chemwaste.htm>.

**Section 7 – Protocol/Procedure (Add lab specific Protocol/Procedure here)**

Click here to enter text.

**NOTE:** Any deviation from this SOP requires approval from PI.

**Section 8 – Documentation of Training (signature of all users is required)**

Prior to conducting any work with acrolein, the Principal Investigator must ensure that all laboratory personnel receive training on the content of this SOP.

**I have read and understand the content of this SOP:**

| **Name** | **Signature** | **Date** |
| --- | --- | --- |
| Click here to enter text. |  | Click here to enter a date. |
| Click here to enter text. |  | Click here to enter a date. |
| Click here to enter text. |  | Click here to enter a date. |
| Click here to enter text. |  | Click here to enter a date. |
| Click here to enter text. |  | Click here to enter a date. |
| Click here to enter text. |  | Click here to enter a date. |
| Click here to enter text. |  | Click here to enter a date. |
| Click here to enter text. |  | Click here to enter a date. |
| Click here to enter text. |  | Click here to enter a date. |
| Click here to enter text. |  | Click here to enter a date. |