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Non-Permit Confined Space Certification


This document certifies that
	[bookmark: Text1]     


has been cleared for a change in status from a Permit Confined Space to a Non-Permit Confined Space provided that the below conditions are met.


[bookmark: Check1]|_|  All entrants/attendants involved in any entry have completed the University’s Confined Space Entry training.


[bookmark: Check2]|_|  All hazards other than atmospheric (e.g., lockout/tag out) can be completed without entry.


[bookmark: Check3]|_|  Any conditions making it unsafe to remove an entrance cover is eliminated before the cover is removed.


[bookmark: Check4]|_|  After removing coverings from horizontal openings, the entrance is promptly guarded by a railing or temporary cover/ barrier to prevent accidental fall through the opening.


[bookmark: Check5]|_|  Before entering space, atmospheric testing is completed with the University’s Confined Space Meter to ensure the following:

1. Oxygen content greater than 19.5% and less than 23.5% (19.5% < O2 < 23.5%)

2. Flammable gases or vapors less than 10% LEL (i.e., Flammbale Gas or Vapors < 10% LEL)

3. Potential toxic air contaminants less than 50 ppm CO (CO < 50 ppm) and less than 20 ppm H2S (H2S < 20 ppm)


[bookmark: Check9]|_|  If the above atmospheric conditions are not met, forced air ventilation may be used if it can maintain them.


Please attach at least 3 previous entry permits for the specific location.
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