**Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Location: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**SAFE GRAIN STORAGE AND HANDLING FOR YOUTH/BEGINNING WORKERS**

1. Which of the following can be considered an agricultural confined space?

1. Grain bin
2. Manure storage facilities
3. Grain transport vehicle (GTVs)
4. All of the above

2. What is the most significant hazard of entering a grain bin and walking on free flowing grain?

1. Amputation
2. Fall
3. Entrapment/suffocation
4. Electrocution

3. If a co-worker is entrapped in a grain bin, the first step I should take is?

1. Enter the bin and attempt to pull him/her out by hand
2. Call 911
3. Shut down energized unloading equipment
4. Throw the victim a rope

4. One out of five victim of flowing grain entrapment is:

1. Under the age of 10
2. Over the age of 60
3. Between age 35-50
4. Under the age of 21

5. My supervisor asked me to clean the residual grain off the walls on the inside of a grain bin, but I don’t think that is safe. Can I say NO?

1. Yes, according to OSHA, I do not need to perform work that I believe is unsafe or that I am not trained to do.
2. No, I cannot say no because I am an employee and need to comply with my employer’s order.